|  |  |
| --- | --- |
| Practice name:  |   |
| Address: |   |
| Contact: |   |
| Phone: | 510-  | Fax: | 510-  |
| Dentists at this office: |   |
| Person responsible for waste hauling: |   |
| Person responsible for amalgam separator: |   |
| USD inspector: |   | Date: |   |
| Re-inspection date to verify corrections of deficiencies: |   |

**1. Amalgam Waste Management**

**Required Waste Management Practices** [ ]  Applicable [ ]  Not applicable

Does office comply?

Yes No N/A

[ ]  [ ]  [ ]  [1a] Do not rinse chair-s ide traps, vacuum screens, and amalgam separator equipment in a sink or other sanitary sewer connection. [USD Ordinance 36 Section 2.02 (b) (1)]

[ ]  [ ]  [ ]  [1b] Properly recycle or dispose of chair-side traps, vacuum screens, and amalgam separator equipment. [36 Section 2.02 (b) (1)]

[ ]  [ ]  [ ]  [2a] Train staff in proper handling and disposal of amalgam materials and fixer-containing solutions. [36 Section 2.02 (b) (2)]

[ ]  [ ]  [ ]  [2b] Keep record of this staff training. [36 Section 2.02 (b) (2)]

[ ]  [ ]  [ ]  [3] Collect, package, label, store and manage amalgam wastes in accordance with state and local regulations. For example, a practice may use a large well-sealed plastic container to hold used chair-side traps, vacuum screens, amalgam separator wastes, used capsules, extracted teeth, and other amalgam wastes for recycling. [36 Section 2.02 (b) (3)]

[ ]  [ ]  [ ]  [4] Use a vacuum line disinfectant that does not contain bleach or other chlorine-containing disinfectant. [136 Section 2.02 (b) (4)]

[ ]  [ ]  [ ]  [5] Use pre-measured amalgam capsules. Use of bulk mercury is prohibited. [36 Section 2.02 (b) (5)]

Other Comments:

**Required Amalgam Separator** [ ]  Applicable [ ]  Not applicable

|  |  |  |  |
| --- | --- | --- | --- |
| Manufacturer: |   | Model: |   |
| Vendor: |   | Date installed: |   |
| Separator location: |   | Maintenance by: |   |
| Amalgam waste hauler: |   |
| Separator waste hauler: |   |

Does office comply?

Yes No

[ ]  [ ]  [6a] Install an ISO-11143 Certified Amalgam Separator Device in the office vacuum system. This device is certified as removing a minimum of 95% of amalgam. [36 Section 2.02 (c) (2)]

[ ]  [ ]  [6b] The amalgam separator system is certified at flow rates comparable to the actual flow rate of the office's vacuum suction system. [36 Section 2.02 (c) (2)]

[ ]  [ ]  [6c] Neither the separator device nor the related plumbing include an automatic flow bypass. [36 Section 2.02 (c) (2)]

[ ]  [ ]  [7] Amalgam separator is operated and maintained in accordance with manufacturer's recommendations. [36 Section 2.02 (c) (4)]

 Date of last service:

[ ]  [ ]  [8] Amalgam separator waste is disposed of using an authorized hauler, recycler or disposal facility. [36 Section 2.02 (b) (3)]

Comments Regarding Amalgam Separator:

## 2. Other Hazardous Waste Management

**Type of X-ray** [ ]  Film [ ]  Digital

Does office comply?

Yes No N/A

[ ]  [ ]  [ ]  [8a] Collect, package, label, store and manage x-ray chemical wastes in accordance with state and local regulations. [36 Section 2.01.2 (d), i)]

[ ]  [ ]  [ ]  [8b] Collect, package, label, store and manage x-ray film and lead foil wastes in accordance with state and local regulations. [36 Section 2.01.2(d), (i)]

[ ]  [ ]  [ ]  [9] Collect, package, label, store and manage glutaraldehyde in accordance with state and local regulations. [36 Section 2.01.2 (d), (i)]

Comments Regarding Other Wastes: